**How to switch touch device driver**  
  
1. Decompress the zip file.  
2. Click the “DriverPatch.exe”  
  
一張含有 文字, 軟體, 數字, 字型 的圖片

自動產生的描述  
  
3. Please click “Yes “ button , if the “User Account Control” dialog is pop-up.  
  
一張含有 文字, 電子產品, 螢幕擷取畫面, 陳列 的圖片

自動產生的描述  
  
4. If your system has touch device that installed with eGalaxTouch driver, you will see a message like the below picture. And the tool starts to switch touch device with inbox (native) driver.  
  
If success, the window will close automatically.  
一張含有 文字, 螢幕擷取畫面, 字型, 軟體 的圖片

自動產生的描述  
  
If the tool cannot find the EETI touch device with eGalaxTouch driver or the Windows is not Windows 10, you will see an error message like below picture.  
一張含有 文字, 螢幕擷取畫面, 字型, 軟體 的圖片

自動產生的描述  
  
  
After apply the new driver, the mulit-touch device should work correctly.  
If you encounter any problem, please contact [touch\_fae@eeti.com](mailto:touch_fae@eeti.com) for supporting.